How to install:

- Copy "ikatube" directory to the mpv config directory (like /Users/user/.config/mpv/ikatube)
- Copy "ikatube2-arm64.so" (Apple Silicon) or "ikatube2-x86_64.so" (Intel) to the mpv script directory (like /Users/user/.config/mpv/scripts/ikatube2-arm64.so)

How to use:

- Press F12 to toggle ikatube interface overlay
- ESC can also close the overlay
- Overlay can be toggled with "script-message ikafb-toggle" command
- Edit the config file in the copied ikatube directory (like /Users/user/.config/mpv/ikatube/ikatube.json)
- Playing the video will load it in the current mpv host, no new mpv process will be created
